# SPDX-License-Identifier: GPL-2.0-or-later

#

# Example OpenOCD configuration file for ESP32-WROVER-KIT board.

#

# For example, OpenOCD can be started for ESP32 debugging on

#

# openocd -f board/esp32-wrover-kit-3.3v.cfg

#

# Source the JTAG interface configuration file

source [find interface/ftdi/esp32\_devkitj\_v1.cfg]

set ESP32\_FLASH\_VOLTAGE 3.3

# Source the ESP32 configuration file

source [find target/esp32.cfg]